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Construction Environmental Management Plan including Biodiversity

For the planning application ref of; BN/64/26/PL

11/06/2026

a) Risk assessment of potentially damaging construction activities

The site has been assessed in terms of ecological interest and there is currently the potential for a bat roost in the existing property. A European Bat Licence will be applied for in respect of the soft stripping of roof materials under Ecological Supervision. The site is considered suitable for registration under Bat Mitigation Class Licence (BMCL). It should be noted that the site lies within the SAC Singleton and Cocking Tunnels and appropriate enhancement is noted in the BERS. The proposed construction zone is located within the wider conservation zone of the Singleton and Cocking Tunnels SAC. A series of avoidance measures have been proposed which ensure that the development has no adverse effect upon the conservation features.

As the area affected by the scheme consist of land of low ecological value as existing storage buildings and will be removed under ecological supervision and the ground surface bare prior to construction activities thus there will be no risk of disturbance to ground nesting birds or other wildlife.


b) Identiﬁcation of ‘biodiversity protection zones’
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c) Practical measures (both physical measures and sensitive working practices) to avoid or reduce impacts during construction


The following should also be utilised during construction works:


1. The placement of gully protection
2. Scrapping of roads to remove silt
3. Speed ramps to slow Traffic down
4. The placement of topsoil and planting at the earliest opportunity to control run of
5. Avoid washing out next to soakaway/gullies

6. General good housekeeping
7. No light pollution during out of hours


d) The location and timing of sensitive works to avoid harm to biodiversity features


The agreed day time working hours regime (8.00am – 6.00pm Monday to Friday) (8.00am – 1.00pm Saturday) will ensure there is no need for artiﬁcial lighting therefore there will be no signiﬁcant disturbance. There will be no need for any loss or disturbance to habitats or potentially supporting nesting birds.


e) The times during construction when specialist ecologists need to be present on site to oversee works

Demolition/Soft Strip


f) Responsible persons and lines of communication


Our Ecologist Consultant will be nominated as ecological clerk of works. This role will ensure compliance with the CEMP and in order to ensure that there is no deterioration in the health and condition of surrounding trees/hedges.


g) The role and responsibilities on site of an ecological clerks of works


The role of the ECoW will be to control the following:
· The CEMP
· Environmental Plan
· Construction Method Statements
· Permits to work/dig
· Toolbox Talks
· Attendance/Input in Site Meetings


h) The use protective fences, exclusion barriers and warning signs


As the above plan all trees/hedges will be protected by suitable a BS compliant (BS 5837:2012) tree protection barrier during construction period.
Appropriate ‘No Access: Biodiversity Protection Zone’ warning signage will be installed on the barrier fencing.





i) Other measures to be taken into account whilst construction is taking place


Site toolbox talks will still be presented to our workforce discussing all protected species including dormice, bats and etc. Should any protected species be seen on site the process will be that ECoW is immediately informed and all works on site are stopped and our Ecologist or Governing Body is informed and invited down to site.
The Biodiversity Exclusion Zone will offer potential foraging areas for dormice.

1. the anticipated number, frequency and types of vehicles used during construction.

Types of Vehicles:

Tipper Lorries (Length 8.2m, Width 2.5m, Height 2.9m)
Concrete Lorries (Length 8.4m, Width 2.4m, Height 4.0m)
Flat Bed Trucks (Length 8.0m, Width 2.1m)
Skip Lorries (Length 6.3m, Width 2.9m, Height 2.9m)
Transit Vans (Length 5.3m, Width 2.0m, Height 2.5m)

Number & Frequency of Vehicles:

	
	Demolition Phase
	Construction Phase

	Tipper Lorries
	2
	2

	Concrete Lorries
	0
	0-1

	Flat bed Trucks
	0
	2

	Skip Lorries
	1-2
	0-1

	Daily Total:
	2-3
	4-6





1. the provision made for the parking of vehicles by contractors, site operatives and visitors.

A logistic plan will indicate contractor, operative and visitor parking

1. the loading and unloading of plant, materials and waste.

Delivery vehicles are to access the site via Greenacre Gardens and utilise the site access gates as indicated on the logistic plan.

Off loading or loading of materials will be carried out manually or by mechanical forklift.

Deliveries will be undertaken on ‘just in time’ basis with all deliveries needing to be booked in 48 hours notice, this will assist in storing the minimum amount of materials on site

All deliveries will be supported by a traffic marshall.

1. the storage of plant and materials used in construction of the development.

A logistic plan will indicate material storage areas. 

1. the erection and maintenance of security hoarding.

This will either be 2.0m security HERAS fencing or ply hoarding

1. the provision of road sweepers and/or wheel washing facilities to mitigate the impact of construction upon the public highway

Roads and footways will be swept as required to remove any spoil or debris deposited on the highway.

A jet wash will be on site for wheel washing and road sweepers will be booked as required.







1. measures to control the emission of dust and dirt during construction, to include where relevant sheeting of loads, covering and dampening down stockpiles

During the demolition phase all arisings will be dampened down to ensure dust and dirt pollution does not occur.

All deliveries and muck away to and from site will be sheeted.

Stockpiled material will be dampened down or sheeted if required.

1. measures to control the emission of noise during construction.

All compression tools will be fitted with silencers to reduce noise levels.

All plant and equipment will be selected to ensure it is correct for the task, the timing and duration of the operation will be considered to ensure it does negatively impact neighbours.

1. details of all proposed external lighting to be used during construction and measures used to limit the disturbance of any lighting required. Lighting shall be used only for security and safety.

There will only be security lighting on the site cabins and security cameras

1. appropriate storage of fuel and chemicals, in bunded tanks or suitably paved areas

All fuel, oil and chemicals shall be stored in accordance with the Manufacturer’s recommendations within bunded tanks and lockable COSHH store.

1. waste management including litter and prohibiting burning of materials/waste.

No burning of materials/waste will happen on site.

As required the site foreman/labourer will carry out a litter pick up in and around the site if applicable.

All waste will be segregated prior to landfill with an implementation of re-use and recycling strategy of reducing landfill waste by circa 90%.

Our supply chain partners monitor, report and audit of waste produced on site.







j) Construction Environment Management in relation to :


	
Air Quality

	Pre-works

	All construction facilities erected on site must be designed and operated to minimise the emission of smoke, dust, cement dust and other substances into the atmosphere.

	Works phase

	Vehicular access will be kept to sealed roads wherever possible or to designated site access points

	A 5mph speed limit shall be imposed on all vehicles within the construction site,
including haul roads.

	A water hose for spraying to reduce dust generation from exposed surfaces will be
available at all times during the contract.

	Water shall be available at all times for spraying all exposed areas to reduce dust
generation.

	The area to be disturbed for excavations will be minimised

	Stockpiles, access roads and work areas will be watered down or covered



	Excess spoil will be placed in skip bins or covered stockpiles, reused on-site or disposed of-site.

	Materials transported in open trucks will be covered to prevent generation of dust.

	The tailgates of all vehicles transporting material from the construction site will be securely ﬁxed prior to loading and immediately after unloading.

	Complete landscaping and revegetation as soon as possible following building activities

	Ensure that no disturbance of the nature strip occurs between the site and the roadway

	Machinery will be well maintained with no noxious emissions and not left idling when not in use.

	Exhaust systems and engines for plant/equipment will be maintained according to the manufacturers’ speciﬁcations and regularly monitored to ensure that exhaust emissions are satisfactory (smoke for no longer than 10 seconds). Periodic visual checks will be made on exhaust system emissions

	The burning of timber and other combustible materials is not permitted on site at any time.

	If winds are high and the works are creating high levels of dust that are likely to cause discomfort to local residents or a safety hazard to traffic or work personnel, the works shall be modified or stopped until the dust hazard is eliminated or is
reduced to an acceptable level.

	Post-works phase

	All exposed soil areas shall be stabilised and revegetated as soon as possible on
completion of works to prevent the generation of dust.





	
Fuels and Chemicals

	Works phase

	A hazardous substance register is kept on site (Form F04)

	Where fuel, oil or other chemicals are to be stored on site, a secure, lockable and floored area will be provided before any of these substances are accepted on site. This area will be imperviously bunded with a capacity to contain not less than 110% of the volume of the largest container. This bunded area is monitored weekly and drained when required, to ensure that bund capacity is maintained, by
pumping out to an oil–water separator.

	Relevant Material Safety Data Sheets (MSDSs) are available on-site for all
chemicals used or stored on site.

	All chemicals are stored in accordance with the manufacturer’s instructions and
the MSDS



	In the event of spillage of hydrocarbon products such as fuels and/or chemicals, on-site spill containment equipment/kits will be used to contain spills and cleaned
in accordance with the MSDS requirements.

	Fuel, oil and chemicals will be used in a bunded area.

	A 50-litre container of spill absorbent will be retained within the site working area
to be used for emergency spills of fuel, oil or other chemicals.

	Ensure that any spills or accidents on site that are likely to cause pollution are
managed as per this plan

	If stormwater discharges from bunded fuel or hazardous storage areas are
required, records are kept of water quality checks, discharges and remedial actions.

	If drums of chemicals and fuels must be used outside a bunded area, a spill kit will be readily available nearby, the drums will not be left unattended, and they will be
returned to the bunded area for storage overnight.

	If an Environmental Incident occurs on site, the Incident Report form F09 will be
completed and forwarded to the Client.

	If refuelling or maintenance cannot take place at this site, temporary bunding will
be provided and adequate spill kits kept readily available.

	Refuelling operations will not be left unattended while in progress.







	
Noise Management

	Pre-works phase

	The site compound will be located the furthest distance from adjacent residences
as practicably possible.

	Works phase

	Construction noise is to be confined to 8am to 6 pm Monday to Friday and 9am to
1pm on Saturdays. No work will be undertaken on Sundays or Public Holidays.

	Noise mitigation measures if required will be implemented during construction to ameliorate the effects of construction noise. Noise generated from construction, maintenance or demolition of a building or other structure should not exceed (75dba), measured at the site of a nearest sensitive receptor on the East and West
side of the site.

	No blasting will be permitted during construction

	All plant and equipment used on this job is operated by appropriately trained staff in accordance with regulations and is regularly maintained and serviced by
qualified staff.

	All plant and equipment used on site will comply with EPA Guidelines.

	Equipment not in use will not be left idling.

	All stationary and mobile equipment will be fitted with residential type silencers.








Signed by 


J Shopland
11/06/26
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