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Foundation & Substructure
The sub-base will be gravel on compacted earth (existing)
The base is supplied along with the greenhouse to ensure it is stable and level.  It is a 12.8cm steel base (4980mm x 2510mm)


Frame & Superstructure
Primary framing is powder coated aluminium in green or black rather than bright aluminium to reduce the visual impact of the greenhouse.
For dimensions please refer to revised elevation plans.
Structural fittings are also back coated aluminium.


Glazing & Enclosure
Roof and wall single glazing is 3mm toughened safety glass.


Doors & Ironmongery
Doors are of the same materials as those outlined above (3mm toughened safety glasses and black aluminium frames).



