Following our refused replacement window application, we reviewed the comments and took your advice, engaging a bespoke joiner to conduct a survey of the windows. He was a recommendation from the previous owner and has already undertaken extensive repair work for them on our house. The aim of this survey was to identify what further maintenance and repairs could be undertaken to the existing windows to address issues with rot, draughts and general disrepair. His expert view was that they were beyond repair and needed to be replaced, in line with the advice given to the previous owners some 10+ years ago.
Our revised proposal involves installing completely bespoke windows that will aesthetically match the existing, to include individual glazed pains with proper, structural dividing bars that match the design and dimensions of the existing windows. This would ensure that there is no visible impact and is intended to be in keeping with the windows that are currently installed.
As per the recommendation from the heritage/conservation society in response to our previous submission, our revised proposal will also utilise heritage slim sightline (12mm/14mm) double glazing rather than the standard 24-28mm thickness. As well as the obvious environmental benefits, this will also allow us to remove the secondary glazing currently installed internally which is also in need of repair and clearly not in keeping with the heritage of the building or internal aesthetic. 
We are committed to investing in maintaining our home through sympathetic repair and or replacement and want to ensure the proposal addresses the concerns of conservation whilst still meeting our needs.

