WORKPLACE RISK ASSESSMENT FORM

	Contract
	Wick Street, Toilet Block, Littlehampton BN17 6JL
	Location
	Wick Street, Toilet Block, Littlehampton BN17 6JL
	Date:
	14/10/2025 T1

	Assessor
	Clive Wilsdon

	Operation
	Demolition of brick and concrete toilet block
	Ref No:
	RA/001 

	



	
HAZARDS
	
PERSONS AFFECTED
	
RISK
	
CONTROL MEASURES
(List control measures that are provided and those required)
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Pedestrian Management
	

Third Parties – GT & TW personnel
	


4
	


5
	


20
	1. The works area will be excluded with warning signage clearly dis- 
             played.
2. Protective screens will be put in place around demolition zone to segregate the area and to protect others from the works - these will consist of Heras Panels and pedestrian barriers fixed together.
3. Marshals will manage all third-party pedestrian safe access when requested.
4. When third party access is required, the Marshal will signal for  
plant to cease works and the machine placed in the rest position.
5. A safe route will be cleared and access then facilitated.
6. Barriers will form red zone for demolition area and amber zone for plant operating zone
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	Plant Access
	3rd Party Property 
	3
	4
	12
	1. The road will be adequately protected using proprietary, standard solution materials for safe plant and vehicle access.
2. Banksman in radio contact with each other, will guide transport to the TOCOP area at walking pace, below 5MPH.
	1
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	4

	


Noise Dust Vibration and flying debris.
	


Operatives and sensitive receptors in proximity to the works.
	


5
	


4
	


20
	1. Install debris netting on heras fencing to act as a screen 
2. Demolition works will be undertaken in keeping with best practice procedures.
3. Where practicable a hydraulic pulveriser will be used to minimise noise, vibration and flying debris.
4. The works area will be kept damped down at all times during the demolition process using on board hoses attached to nearby potable water source.
5. Regular monitoring will be undertaken by the MSL supervisor with readings recorded
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Plant Pedestrian Segregation.







Plant Pedestrian Segregation.
	
Operatives & Third Parties






Operatives & Third Parties
	









5
	









5
	









25
	1. Demolition plant will work within an exclusion zone, with warning signage clearly displayed.
2. Pedestrian barriers will be used to separate moving plant and opearatives
3. The ‘thumbs up’ procedure will be adhered to:
Before access into a demolition working zone, the machine operator must be first made aware of access being required. 
· This can be a verbal signal via 2-way radio or a hand signal from the banks man.
· Having been signaled/notified, the machine operator will make safe the area of demolition and place the machine in the rest position.
· The operator will then signal back with a ‘thumbs up’.
· In the case of demolition debris being present, a safe pedestrian access route must be cleared.
· Access to the works area can then proceed.
· No works to recommence until the third party is back outside of the exclusion zone, it’s been secured and the banksman gives a ’thumbs up’ to the operator to proceed.
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Uncontrolled Collapse
	
Operatives, Third Parties, TW Infrastructure
	

5
	

5
	

25
	1. A visual and physical inspection will be carried out forming openings in roof at junction of wall to determine best sequence of demolition.
2. Multi Processing jaws will be used to reduce vibration and flying debris.
3. The demolition works will be supervised at all times by a trained and competent person.
4. The works will be ceased immediately in the event of the structure being different to that anticipated and an alternative methodology will be developed if needed.
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Contact with Sewage, Weil’s disease, Contaminated Materials / Bacterial Infection 
	





All Site Personnel

	












3
	












4
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1. Full length PPE must be worn at all times on site – Long Sleeved Hi Vis (Orange), Over Trousers (Orange), S3 Safety Boots, Safety Spectacles and Gloves that are specific to the task being carried out.
2. Hygiene procedures to be strictly maintained: 

             Thoroughly wash hands immediately after leaving the  
             site area using soap and hot water at the end of each working  
             shift.

             Do not eat, drink, smoke or vape (in the appropriate designated  
             areas) without having first washed your hands thoroughly.

             Report to the first aid post immediately if affected by cuts or   
             abrasions encountered during the working shift.

              Ensure cuts/abrasions are cleaned and covered before going 
              back out onto site.

              In the event of developing flu-like symptoms, report immediately 
              to your GP.
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Plant
	


Operatives & Third Parties
	


4
	


5
	


20
	1. All plant will have a valid and in date certificate of thorough 
       inspection.
2. Only trained and competent CPCS personnel will operate plant.
3. All plant will operate from within an exclusion zone with warning signs clearly displayed.
4. All excavators will work with a Slinger Signaller/Plant Banksman always accompanying.
5. No persons will attempt to enter an exclusion zone without first gaining permission from the driver and the machine is placed in the rest position (thumbs up).
	


1
	


5
	


5

	

COSHH
	

Operatives
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4
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	1. COSHH assessments will be carried out for all materials being used:
· Lithium Grease, Diesel, Hydraulic Oil,
2. A spill kit will be located directly adjacent to the works, just outside of the exclusion zone.
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Damage to property 
	








Site Deliveries/Site Traffic & Plant Management
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	1. All site personnel will be briefed on the TMP at induction and before going onto site.
2. MSL access into site will be always managed during deliveries to prevent other contractor’s traffic queuing on the highway. 
3. All plant will operate with warning beacons on. 
4. Plant/Pedestrian separation will be implemented by plant exclusion zones and separate excluded routes for pedestrians.
5. Roads will be maintained swept clean at all times following deliveries and/plant movements.
6. Transport coming to or leaving site must be clean and clear of mud or debris. 
7. Plant must be cleaned down before tracking out of site for loading onto transport.
8. Plant arriving to site must have been cleaned down prior to loading of the delivery transport.
9. Gritting materials will be kept on site and made available for colder conditions.
	









1
	









4
	









4

	



Slips and Trips & Falls
	


Operatives
	


5
	


4
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	1. The works will be carried out in an excluded area with warning signage clearly displayed.
2. Hoses will be run responsibly, clear of pedestrian routes and cut to a size that accommodates the works.
3. The works area will be swept clear daily of small debris or existing mosses/weeds that could otherwise present a potential for slip when wet.
4. The demolition zone will be excluded from pedestrian access.
5. Only pedestrian safe routes to be used when walking across site.
6. Barriers and signage will form exclusion zones for plant and pedestrians
7. Ramps will be formed where access by plant and pedestrians is required, open edges to voids and ramps will be lined with barriers and/or heras fencing
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Manual Handling
	



Operatives
	




5
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	1. Manual handling will always be avoided where an alternative method is available (by machine, flat bed trolley etc.)
2. Team lifting will be used to lift/carry bulky or unwieldly objects.
3. No person to lift any weight they do not feel comfortable lifting.
4. Where there’s repetitive lifting or a rate imposed by process, then frequent rest breaks should be taken and/or rotation of personnel.
5. Operatives with a history of musculoskeletal complaints or disorders should be excluded from manual handling activities.
8. A manual handling assessment will be carried out prior to any lifting or carrying activities commencing.
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Hot Works 
	





Operatives & Third Parties
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	1. Works to be carried out by a trained and competent operative only.
2. RPE appropriate to the task, flame proof coveralls, burners boots, tinted visor and leather gauntlets must be worn.
3. All equipment must be entered on to the PUWER register and checked before each & every use; a thorough, documented inspection will be carried out weekly in compliance with PUWER.
4. Bottles must be stored away from the works area in lockable cages when not in use, appropriate warning signage must be clearly displayed.
5. An appropriately stocked fire point must be located adjacent to the bottle cage.
6. Propane and Oxygen bottle cages must be kept separated at a distance not less than 3M.
7. Hoses, regulators and nozzles must all be checked and in good condition before each use, pressure gauges must be fitted.
8. Flash back arrestors must be fitted.
9. Hot work permits to be issued daily after hot works area inspection by a competent person and signed by MSL and GT supervisor.
10. Hot works to cease 2 hours prior to end of shift and the area quenched with water before the 2-hour fire watch commences.
11. The hot works permit must be closed out daily after the fire watch period has completed and signed by MSL and GT supervisor.
12. When in use oxy/propane bottles must be chained and fixed upright on a dedicated bottle trolley.
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	Assessor Signature   
Date 15-10-2025


	NO OPERATION MUST BE CARRIED OUT UNTIL ALL THE CONTROLS MEASURES IDENTIFIED IN THIS ASSESSMENT ARE IN PLACE

[image: ]Likelihood
How often could the hazard occur? Consider the task, frequency, duration, method of work, 
employees involved.


Severity
How serious would the hazard’s effects be if 
realised? Consider the type of hazard, biological, ergonomic, physical and chemical.


Risk = Likelihood x Severity 

E.g. Likelihood (4) X Severity (3) = 12 HIGH RISK









	LOW RISK
(Score 1-6)

	May be acceptable, however, review task to see if risk can be reduced further.

	MEDIUM RISK
(Score 8-10)
	Where possible the task should be refined to take account of the hazards involved or the risks should be reduced further prior to task commencement.

	HIGH RISK
(Score 12-25)
	Task must not proceed.  Further control measures to be put in place to further reduce risk.  The controls should be re-assessed for adequacy prior to work commencement.
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